# 
#
# For more info:
# https://github.com/arduino/Arduino/wiki/Arduino-IDE-1.5---3rd-party-Hardware-specification

name=STM32F1 Boards (STM32duino.com)
version=0.1.2

compiler.warning_flags=-w -DDEBUG_LEVEL=DEBUG_NONE
compiler.warning_flags.none=-w -DDEBUG_LEVEL=DEBUG_NONE
compiler.warning_flags.default=-DDEBUG_LEVEL=DEBUG_NONE
compiler.warning_flags.more=-Wall -DDEBUG_LEVEL=DEBUG_FAULT
compiler.warning_flags.all=-Wall -Wextra -DDEBUG_LEVEL=DEBUG_ALL

# compiler variables
# ----------------------
compiler.path={runtime.tools.arm-none-eabi-gcc.path}/bin/
compiler.c.cmd=arm-none-eabi-gcc
compiler.c.flags=-c -g {build.flags.optimize} {compiler.warning_flags} -std=gnu11 -MMD -ffunction-sections -fdata-sections -nostdlib --param max-inline-insns-single=500 -DBOARD_{build.variant} -D{build.vect} -DERROR_LED_PORT={build.error_led_port} -DERROR_LED_PIN={build.error_led_pin} 
compiler.c.elf.cmd=arm-none-eabi-g++
compiler.c.elf.flags={build.flags.optimize} -Wl,--gc-sections {build.flags.ldspecs}
compiler.S.cmd=arm-none-eabi-gcc
compiler.S.flags=-c -g -x assembler-with-cpp -MMD
compiler.cpp.cmd=arm-none-eabi-g++
compiler.cpp.flags=-c -g {build.flags.optimize} {compiler.warning_flags} -std=gnu++11 -MMD -ffunction-sections -fdata-sections -nostdlib --param max-inline-insns-single=500 -fno-rtti -fno-exceptions -DBOARD_{build.variant} -D{build.vect} -DERROR_LED_PORT={build.error_led_port} -DERROR_LED_PIN={build.error_led_pin} 
compiler.ar.cmd=arm-none-eabi-ar
compiler.ar.flags=rcs
compiler.objcopy.cmd=arm-none-eabi-objcopy
compiler.objcopy.eep.flags=-O ihex -j .eeprom --set-section-flags=.eeprom=alloc,load --no-change-warnings --change-section-lma .eeprom=0
compiler.elf2hex.flags=-O binary
compiler.elf2hex.cmd=arm-none-eabi-objcopy
compiler.ldflags={build.flags.ldspecs}
compiler.size.cmd=arm-none-eabi-size
compiler.define=-DARDUINO=                            

# this can be overriden in boards.txt
build.f_cpu=72000000L
build.mcu=cortex-m3
build.common_flags=-mthumb  -march=armv7-m -D__STM32F1__ -DARDUINO_ARCH_STM32
build.variant_system_lib=libmaple.a
## LED stuff is not really used but is still required in the code
build.error_led_port=GPIOB
build.error_led_pin=1
build.cpu_flags=
build.hs_flag=
build.upload_flags=
build.flags.optimize=-Os
build.flags.ldspecs=
build.extra_flags= {build.upload_flags} {build.cpu_flags} {build.hs_flag} {build.common_flags}



# These can be overridden in platform.local.txt
compiler.c.extra_flags=
compiler.c.elf.extra_flags="-L{build.variant.path}/ld"
compiler.cpp.extra_flags= 
compiler.S.extra_flags=
compiler.ar.extra_flags=
compiler.elf2hex.extra_flags=


compiler.libs.c.flags="-I{build.system.path}/libmaple" "-I{build.system.path}/libmaple/include" "-I{build.system.path}/libmaple/stm32f1/include" "-I{build.system.path}/libmaple/usb/stm32f1" "-I{build.system.path}/libmaple/usb/usb_lib" 




# USB Flags
# ---------
## build.usb_flags=-DUSB_VID={build.vid} -DUSB_PID={build.pid} -DUSBCON '-DUSB_MANUFACTURER={build.usb_manufacturer}' '-DUSB_PRODUCT={build.usb_product}'

# Default usb manufacturer will be replaced at compile time using
# numeric vendor ID if available or by board's specific value. 
## build.usb_manufacturer="Unknown"


# build patterns
# ---------------------

## Compile c files
recipe.c.o.pattern="{compiler.path}{compiler.c.cmd}" {compiler.c.flags} -mcpu={build.mcu} -DF_CPU={build.f_cpu} -DARDUINO={runtime.ide.version} -DARDUINO_{build.board} -DARDUINO_ARCH_{build.arch} {compiler.c.extra_flags} {build.extra_flags} {compiler.libs.c.flags} {includes} "{source_file}" -o "{object_file}"

## Compile c++ files
recipe.cpp.o.pattern="{compiler.path}{compiler.cpp.cmd}" {compiler.cpp.flags} -mcpu={build.mcu} -DF_CPU={build.f_cpu} -DARDUINO={runtime.ide.version} -DARDUINO_{build.board} -DARDUINO_ARCH_{build.arch} {compiler.cpp.extra_flags} {build.extra_flags} {build.cpu_flags} {build.hs_flag} {build.common_flags} {compiler.libs.c.flags} {includes} "{source_file}" -o "{object_file}"

## Compile S files
recipe.S.o.pattern="{compiler.path}{compiler.c.cmd}" {compiler.S.flags} -mcpu={build.mcu} -DF_CPU={build.f_cpu} -DARDUINO={runtime.ide.version} -DARDUINO_{build.board} -DARDUINO_ARCH_{build.arch} {compiler.S.extra_flags} {build.extra_flags} {build.cpu_flags} {build.hs_flag} {build.common_flags} {compiler.libs.c.flags} {includes} "{source_file}" -o "{object_file}"

## Create archives
recipe.ar.pattern="{compiler.path}{compiler.ar.cmd}" {compiler.ar.flags} {compiler.ar.extra_flags} "{archive_file_path}" "{object_file}"

## Combine gc-sections, archives, and objects
recipe.c.combine.pattern="{compiler.path}{compiler.c.elf.cmd}" {compiler.c.elf.flags} -mcpu={build.mcu} "-T{build.variant.path}/{build.ldscript}" "-Wl,-Map,{build.path}/{build.project_name}.map" {compiler.c.elf.extra_flags} -o "{build.path}/{build.project_name}.elf" "-L{build.path}" -lm -lgcc -mthumb -Wl,--cref -Wl,--check-sections -Wl,--gc-sections -Wl,--unresolved-symbols=report-all -Wl,--warn-common -Wl,--warn-section-align -Wl,--warn-unresolved-symbols -Wl,--start-group {object_files} "{archive_file_path}" -Wl,--end-group

## Create eeprom
recipe.objcopy.eep.pattern=

## Create hex
recipe.objcopy.hex.pattern="{compiler.path}{compiler.elf2hex.cmd}" {compiler.elf2hex.flags} {compiler.elf2hex.extra_flags} "{build.path}/{build.project_name}.elf" "{build.path}/{build.project_name}.bin"

## Compute size
recipe.size.pattern="{compiler.path}{compiler.size.cmd}" -A "{build.path}/{build.project_name}.elf"
recipe.size.regex=^(?:\.text|\.data|\.rodata|\.text.align|\.ARM.exidx)\s+([0-9]+).*
recipe.size.regex.data=^(?:\.data|\.bss|\.noinit)\s+([0-9]+).*

## Save Compiled Binary
recipe.output.tmp_file={build.project_name}.bin
recipe.output.save_file={build.project_name}.{build.variant}.bin

# Uploader tools
# -------------------

# Upload using Maple bootloader over DFU
tools.maple_upload.cmd=maple_upload
tools.maple_upload.cmd.windows=maple_upload.bat
tools.maple_upload.path={runtime.hardware.path}/tools/win
tools.maple_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.maple_upload.path.linux={runtime.hardware.path}/tools/linux
tools.maple_upload.path.linux64={runtime.hardware.path}/tools/linux64    
tools.maple_upload.upload.params.verbose=-d
tools.maple_upload.upload.params.quiet=
tools.maple_upload.upload.pattern="{path}/{cmd}" {serial.port.file} {upload.altID} {upload.usbID} "{build.path}/{build.project_name}.bin"

#Added tool for generic STM32 upload via serial to Serial Port 1 (pins PA9 and PA10) - note. Boot0 line needs to high on board reset to enable upload via serial
# at the end up the upload the program is automatically run, without the board being reset

tools.serial_upload.cmd=serial_upload
tools.serial_upload.cmd.windows=serial_upload.bat
tools.serial_upload.cmd.macosx=serial_upload
tools.serial_upload.path={runtime.hardware.path}/tools/win
tools.serial_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.serial_upload.path.linux={runtime.hardware.path}/tools/linux
tools.serial_upload.path.linux64={runtime.hardware.path}/tools/linux64
tools.serial_upload.upload.params.verbose=-d
tools.serial_upload.upload.params.quiet=n
tools.serial_upload.upload.pattern="{path}/{cmd}" {serial.port.file} {upload.altID} {upload.usbID} "{build.path}/{build.project_name}.bin"

# stlink upload
tools.stlink_upload.cmd=stlink_upload
tools.stlink_upload.cmd.windows=stlink_upload.bat
tools.stlink_upload.path.windows={runtime.hardware.path}/tools/win
tools.stlink_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.stlink_upload.path.linux={runtime.hardware.path}/tools/linux
tools.stlink_upload.path.linux64={runtime.hardware.path}/tools/linux64
tools.stlink_upload.upload.params.verbose=-d
tools.stlink_upload.upload.params.quiet=
tools.stlink_upload.upload.pattern="{path}/{cmd}"  "{build.path}/{build.project_name}.bin"
 
# blackmagic probe upload
tools.bmp_upload.cmd=arm-none-eabi-gdb
tools.bmp_upload.path={runtime.tools.arm-none-eabi-gcc.path}/bin/
tools.bmp_upload.upload.speed=230400
tools.bmp_upload.upload.params.verbose=
tools.bmp_upload.upload.params.quiet=-q --batch-silent
tools.bmp_upload.upload.pattern="{path}{cmd}" -cd "{build.path}" -b {upload.speed} {upload.verbose} -ex "set debug remote 0" -ex "set target-async off" -ex "set remotetimeout 60" -ex "set mem inaccessible-by-default off" -ex "set confirm off" -ex "set height 0" -ex "target extended-remote {serial.port}" -ex "monitor swdp_scan" -ex "attach 1" -ex "x/wx 0x8000004" -ex "monitor erase_mass" -ex "echo 0x8000004 expect 0xffffffff after erase\n" -ex "x/wx 0x8000004" -ex "file {build.project_name}.elf" -ex "load" -ex "x/wx 0x08000004" -ex "tbreak main" -ex "run" -ex "echo \n\n\nUpload finished!" -ex "quit"

tools.jlink_upload.cmd=jlink_upload
tools.jlink_upload.cmd.windows=jlink_upload.bat
tools.jlink_upload.cmd.macosx=jlink_upload
tools.jlink_upload.path={runtime.hardware.path}/tools/win
tools.jlink_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.jlink_upload.path.linux={runtime.hardware.path}/tools/linux
tools.jlink_upload.path.linux64={runtime.hardware.path}/tools/linux64
tools.jlink_upload.upload.params.verbose=-d
tools.jlink_upload.upload.params.quiet=n
tools.jlink_upload.upload.pattern="{path}/{cmd}" "{build.path}/{build.project_name}.bin"

# HID upload 2.0
tools.hid_upload.cmd=hid_upload
tools.hid_upload.cmd.windows=hid-flash.exe
tools.hid_upload.cmd.macosx=hid_flash
tools.hid_upload.path={runtime.hardware.path}/tools/win
tools.hid_upload.path.macosx={runtime.hardware.path}/tools/macosx
tools.hid_upload.path.linux={runtime.hardware.path}/tools/linux
tools.hid_upload.path.linux64={runtime.hardware.path}/tools/linux64
tools.hid_upload.upload.params.verbose=-d
tools.hid_upload.upload.params.quiet=n
tools.hid_upload.upload.pattern="{path}/{cmd}" "{build.path}/{build.project_name}.bin" {serial.port.file}
